{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["RNXARKK","说明","100章","200章","300章","400章","600章","700章","800章","900章","汇总表"],"not_rendered":{"external_links":1,"defined_names":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RNXARKK","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"说明","index":1,"n_rows":24,"n_cols":1,"rows_kept":24,"flags":["formulas_cached_only"]}
["第五章  工程量清单"]
["    1.工程量清单说明"]
["        1.1 本工程量清单是根据招标文件中包括的、有合同约束力的图纸以及有关工程量清单的国家标准、行业标准、合同条款中约定的工程量计算规则编制。约定计量规则中没有的子目，其工程量按照有合同约束力的图纸所标示尺寸的理论净量计算。计量采用中华人民共和国法定计量单位。"]
["        1.2本工程量清单应与招标文件中的投标人须知，通用合同条款、专用合同条款、技术规范及图纸等一起阅读和理解。"]
["        1.3本工程量清单中所列工程数量是估算的或设计的预计数量，仅作为投标报价的共同基础，不能作为最终结算与支付的依据。实际支付应按实际完成的工程量，由承包人按技术规范规定的计量方法，以监理人认可的尺寸、断面计量，按本工程量清单的单价和总额价计算支付金额；或者根据具体情况，按合同条款第15.4款的规定，由监理人确定的单价或总额价计算支付额。"]
["        1.4工程量清单各章是按第七章“技术规范”的相应章次编号的，因此，工程量清单中各章的工程子目的范围与计量等应与“技术规范”相应章节的范围、计量与支付条款结合起来理解或解释。"]
["        1.5对作业和材料的一般说明或规定，未重复写入工程量清单内，在给工程量清单各子目标价前，应参阅第七章“技术规范”的有关内容。"]
["        1.6工程量清单中所列工程量的变动，丝毫不会降低或影响合同条款的效力，也不免除承包人按规定的标准进行施工和修复缺陷的责任。"]
["        1.7图纸中所列的工程数量表及数量汇总表仅是提供资料，不是工程量清单的外延，图纸与工程量清单所列数量不一致时，以工程量清单所列数量作为报价的依据。"]
["     2.投标报价的说明"]
["        2.1工程量清单中的每一子目(有数量）须填入单价或价格，且只允许有一个报价。"]
["        2.2除非合同另有规定，工程量清单中有标价的单价和总额价均已包括了为实施和完成合同工程所需的劳务、材料、机械、质检（自检）、安装、缺陷修复、管理、保险、税费、利润等费用，以及合同明示或暗示的所有责任、义务和一般风险。"]
["        2.3工程量清单中投标人没有填入单价或价格的子目，其费用视为已分摊在工程量清单中其他相关子目的单价或价格之中。承包人必须按监理人指令完成工程量清单中未填入单价或价格的子目，但不能得到结算与支付。"]
["        2.4符合合同条款规定的全部费用应认为已被计入有标价的工程量清单所列各子目之中，未列子目不予计量的工作，其费用应视为已分摊在本合同工程的有关子目的单价或总额价之中。"]
["        2.5承包人用于本合同工程的各类装备的提供、运输、维护、拆卸、拼装等支付的费用，已包括在工程量清单的单价或总额价之中。"]
["        2.6工程量清单中各项金额均以人民币（元）结算。"]
["        2.7暂列金额（不含计日工总额）的数量及拟用子目的说明： 本项目不考虑暂列金额。 "]
["    3.计日工说明:无。"]
["    4.其它说明"]
["         4.1建筑工程一切险的投保金额为工程量清单100章至900章的合计金额(除建筑工程一切险和第三者责任险除外)，保险费率为3.0‰；第三者责任险的投保金额为100万元/次，保险费率为4.0‰，事故次数由承包人自行确定，如出现保险事故保险金不足以补偿损失的，应由承包人负责补偿。上述两项保险承包人应以发包人和承包人的共同名义投保。保险费由承包人报价时列入工程量清单100章内。发包人在接到保险单后，将按照保险单的实际费用直接向承包人支付保险费。除上述工程一切险及第三方责任险以外，所投其他保险的保险费均由承包人承担并支付，不在报价中单列。"]
["         4.2为确保将安全施工措施落到实处，投标人应根据《公路水运工程安全生产监督管理办法》（原交通部令2007年第1号）以及《关于印发<企业安全生产费用提取和使用管理办法>的通知》（财企[2012]16号）的规定，在投标总价中计入安全生产费用，安全生产费用以固定金额形式计入工程量清单第100章中（安全生产费用为招标人公布的最高投标限价的1.5％），投标人在投标报价时不得对该固定金额进行调整。如投标人须在此基础上增加安全生产费用以满足项目施工需要，则投标人应在本项目工程量清单其它相关子目的单价或总额价中予以考虑，发包人不再单独支付。承包人的施工安全生产费用，应当用于施工安全防护用具及设施的采购和更新、安全施工措施的落实、安全生产条件的改善，不得挪作他用。"]
["        4.3本项目房建工程（包括加油站工程）的消防手续及交工后的消防、环保验收工作均由承包人组织完成，其费用包含在相关子目单价中，不另行计量与支付。承包人所采购相关加油设备及材料需经中石油相关部门验收合格后方可使用，由于承包人采购的设备及材料不合格而导致的费用增加，相关风险及增加费用由承包人自行承担。 "]
["        4.4本项目后续的路面技术服务、桩基检测、交安（含机电）检测、桥梁动静载检测、单梁静载试验、房建（含钢结构大棚）检测等工作由承包人委托第三方检测机构进行检测（或通过招标确定），第三方检测机构不得与承包人存在关联关系且必须经监理人及发包人认可。委托第三方检测机构发生的费用由承包人根据相关取费标准在本项目工程量清单相关子目的单价或总额价中予以考虑，发包人不再单独支付。"]
["        4.5根据交通运输部《关于开展高速公路施工标准化活动的通知》（交公路发﹝2011﹞70号）、《内蒙古自治区交通运输厅关于推行高速和一级公路施工标准化管理的实施意见》的要求，承包人驻地建设、工地试验室、场站建设、工程施工、施工便道、便桥等均应满足《内蒙古自治区高速和一级公路施工标准化管理指南（试行）》、《内蒙古自治区高速一级公路工程工地试验室监督管理制度的通知》（内交发﹝2013﹞334号）、本招标文件中技术规范及本项目建设管理办法的相应规定。施工标准化及信息化建设费用，以固定金额形式计入工程量清单第100章中（施工标准化及信息化建设费用为招标人公布的最高投标限价的1.5％），投标人在投标报价时不得对该固定金额进行调整。该费用使用及支付详见技术规范。如投标人须在此基础上增加施工标准化及信息化建设费用以满足项目施工需要，则投标人应在本项目工程量清单其它相关子目的单价或总额价中予以考虑，发包人不再单独支付。"]

{"sheet":"100章","index":2,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[1,0,1,5],[2,0,2,5],[3,4,3,5],[30,0,30,4]],"flags":["formulas_cached_only"]}
["5.1 工程量清单表"]
["工程量清单"]
["清单  第100章  总 则"]
["合同段编号：ZAZCB",{"$nulls":3},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
["101-1","保险费"]
[" -a","按合同条款规定；提供建筑工程一切险","总额",1,0,""]
[" -b","按合同条款规定；提供第三方责任险","次数",null,4000,0]
["102-1","竣工文件","总额",1,null,""]
["102-2","施工环保费","总额",1,null,""]
["102-3","安全生产费\n（按投标控制价上限的1.5%计列）","总额",1,null,""]
["103-1","临时道路修建、养护与拆除(包括原道路的养护费)","总额",1,null,""]
["103-2","临时占地","总额",1,null,""]
["103-3","临时供电设施",{"$nulls":3},""]
[" -a","设施架设、拆除","总额",1,null,""]
[" -b","设施维修","总额",1,null,""]
["103-4","电信设施的提供、维修与拆除","总额",1,null,""]
["103-5","供水与排污设施","总额",1,null,""]
["103-6","临时交通安全设施","总额",1,null,""]
["104-1","承包人驻地建设","总额",1,null,""]
["105-1","施工标准化及信息化建设\n（按投标控制价上限的1.5%计列）","总额",1,null,""]
[107,"联合设计（机电工程）"]
["107-2","联合设计（机电工程）","总额",1,null,""]
["107-5","联合设计图纸（6套中文图纸）\n（机电工程）","项",1,null,""]
[108,"工厂测试与监造（机电工程）","总额",1,null,""]
["118-3","调试（含软件、硬件调试）（机电工程）","项",1,null,""]
["119-3","交工质量检测（机电工程）","总额",1,null,""]
[124,"技术培训（机电工程）","总额",1,null,""]
[]
[]
["清单 第100章合计  人民币(元) ",{"$nulls":4},"","注意事项：此项需E11填入数值方会显示数值"]

{"sheet":"200章","index":3,"n_rows":109,"n_cols":6,"rows_kept":109,"merged":[[0,0,0,5],[1,0,1,5],[108,0,108,4]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第200章 路基"]
["合同段编号：ZAZCB",{"$nulls":4},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
["202-1","清理与掘除",{"$nulls":3},""]
[" -a","清理现场","m2",582755,null,""]
[" -b","砍伐树木","棵",225513,null,""]
[" -c","挖除树根","棵",225513,null,""]
["202-2","挖除旧路面",{"$nulls":3},""]
[" -d","挖除水稳砂砾基层","m3",70364,null,""]
[" -e","铣刨沥青面层","m3",86347,null,""]
[" -f","挖除旧路路面结构层","m3",17691,null,""]
["202-3","拆除结构物",{"$nulls":3},""]
[" -a","钢筋混凝土结构","m3",1679,null,""]
[" -b","混凝土结构","m3",11874,null,""]
[" -c","砖、石及其他砌体结构","m3",33598,null,""]
[" -d","波形钢板护栏","m",34298,null,""]
[" -e","柱式轮廓标","根",1494,null,""]
[" -f","附着式轮廓标","块",780,null,""]
[" -g","柱式线形诱导标","根",336,null,""]
[" -h","附着式线形诱导标","块",88,null,""]
[" -i","里程碑","块",56,null,""]
[" -j","公路界碑","块",552,null,""]
[" -k","单柱标志牌","块",120,null,""]
[" -l","双柱标志牌","块",53,null,""]
[" -m","标线","m2",39640,null,""]
["203-1","路基挖方",{"$nulls":3},""]
[" -a","挖土方","m3",585661,null,""]
[" -b","挖石方","m3",1202562,null,""]
[" -c","挖除非适用材料（不含淤泥）","m3",189210,null,""]
[" -d","挖淤泥","m3",459668,null,""]
["203-2","改河、改渠、改路挖方",{"$nulls":3},""]
[" -a","挖土方","m3",227740,null,""]
["203-3","挖除旧路基土方","m3",140368,null,""]
["203-4","清理土方","m3",36090,null,""]
["204-1","路基填筑（包括填前压实）",{"$nulls":3},""]
[" -b","利用土方","m3",623265,null,""]
[" -c","利用石方","m3",657417,null,""]
[" -e","借土填方","m3",94639,null,""]
[" -g","结构物台背回填砂砾","m3",135105,null,""]
[" -h","锥坡及台前溜坡填土","m3",26395,null,""]
[" -i","锥坡及台前溜坡填砂砾","m3",27908,null,""]
["204-2","改河、改渠、改路填筑",{"$nulls":3},""]
[" -a","利用土方","m3",341381,null,""]
[" -b","利用石方","m3",34198,null,""]
["205-1","软土地基处理",{"$nulls":3},""]
[" -b","换填砂砾","m3",2047,null,""]
[" -c","换填碎石土","m3",258975,null,""]
[" -d","换填片石","m3",424150,null,""]
[" -e","换填碎石","m3",150247,null,""]
[" -i","碎石桩，Φ0.8m","m",72553,null,""]
[" -l","土工格栅","m2",362304,null,""]
[" -o","冲击碾压","m2",249605,null,""]
[" -q","土工布","m2",23562,null,""]
["207-1","边沟",{"$nulls":3},""]
[" -a","土质边沟，梯形：40cm×40cm","m",31100,null,""]
[" -b","M10浆砌片石，矩形：40cm×40cm","m",39718,null,""]
[" -c","M10浆砌片石，矩形：40cm×40cm，有盖板","m",7282,null,""]
[" -d","M10浆砌片石，矩形：60cm×60cm","m",4454,null,""]
[" -e","M10浆砌片石，矩形：60cm×80cm，有盖板","m",6506,null,""]
[" -f","M10浆砌片石，矩形：80cm×80cm","m",120,null,""]
[" -g","M10浆砌片石，梯形：顶宽280cm，底宽80cm，深80cm","m",45,null,""]
["207-2","排水沟",{"$nulls":3},""]
[" -a","M10浆砌片石，矩形：40cm×40cm","m",106128,null,""]
[" -b","M10浆砌片石，矩形：40cm×40cm，有盖板","m",9223,null,""]
[" -c","M10浆砌片石，矩形：60cm×60cm","m",15849,null,""]
[" -d","M10浆砌片石，梯形：顶宽320cm，底宽80cm，深80cm","m",1943,null,""]
["207-3","截水沟",{"$nulls":3},""]
[" -a","M10浆砌片石，矩形：40cm×40cm","m",9447,null,""]
[" -b","M10浆砌片石，矩形：60cm×60cm","m",840,null,""]
["207-4","急流槽",{"$nulls":3},""]
[" -a","M10浆砌片石","m3",796,null,""]
[" -b","C30现浇混凝土","m3",1651,null,""]
["207-9","碎砾石渗沟","m",710,null,""]
["207-10","改沟",{"$nulls":3},""]
[" -a","M10浆砌片石，矩形1200cm×150cm","m",305,null,""]
[" -b","M10浆砌片石，矩形2000cm×150cm","m",995,null,""]
["208-1","植物护坡",{"$nulls":3},""]
[" -a","种草","m2",469449,null,""]
[" -b","三维网植草","m2",85636,null,""]
["208-3","护坡",{"$nulls":3},""]
[" -a","拱形骨架护坡，M10浆砌片石","m3",103072.9,null,""]
[" -c","满砌护坡，M10浆砌片石","m3",7854.8,null,""]
["208-4","预制混凝土块护坡",{"$nulls":3},""]
[" -b","拱形骨架护坡，C30混凝土","m3",4116.5,null,""]
["209-3","挡土墙、围墙",{"$nulls":3},""]
[" -a","M10浆砌片石","m3",5440.7,null,""]
[" -b","C25片石混凝土","m3",948.7,null,""]
[" -c","C25素混凝土","m3",1607.7,null,""]
["209-4","护肩墙",{"$nulls":3},""]
[" -a","M10浆砌片石","m3",686.3,null,""]
[" -b","C30混凝土","m3",343.1,null,""]
[" -c","带肋钢筋（HRB335、HRB400）","kg",4189.5,null,""]
["212-5","主动网防护","m2",9947,null,""]
["215-1","河床铺砌",{"$nulls":3},""]
[" -a","M10浆砌片石","m3",1605.6,null,""]
["215-2","导流坝",{"$nulls":3},""]
[" -a","M7.5浆砌片石","m3",360,null,""]
[" -b","M10浆砌片石","m3",556.8,null,""]
[" -c","填筑土方","m3",2619,null,""]
["215-5","锥坡",{"$nulls":3},""]
[" -a","M10浆砌片石","m3",6659.5,null,""]
[" -b","预制C20混凝土空心六棱砖","m3",1226.6,null,""]
["215-6","踏步",{"$nulls":3},""]
[" -a","M10浆砌片石","m3",1180.6,null,""]
[" -b","C20混凝土","m3",184.6,null,""]
["215-7","石笼","m3",2045.5,null,""]
[{"$nulls":5},""]
["清单  第200章合计  人民币(元)",{"$nulls":4},0]

{"sheet":"300章","index":4,"n_rows":55,"n_cols":6,"rows_kept":55,"merged":[[0,0,0,5],[1,0,1,5],[54,0,54,4]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第300章 路面"]
["合同段编号：ZAZCB",{"$nulls":4},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
["302-2","砂砾垫层",{"$nulls":3},""]
[" -a","厚200mm","m2",620103,null,""]
["304-1","水泥稳定碎石底基层",{"$nulls":3},""]
[" -a","厚170mm","m2",244523,null,""]
[" -b","厚180mm","m2",72249,null,""]
[" -c","厚200mm","m2",601686,null,""]
["304-3","水泥稳定碎石基层",{"$nulls":3},""]
[" -a","厚200mm","m2",578881,null,""]
[" -b","厚340mm","m2",235629,null,""]
[" -c","厚360mm","m2",67900,null,""]
["304-4","18cm厚冷再生水稳基层","m2",141588,null,""]
["307-1","沥青稳定碎石基层（ATB-30）",{"$nulls":3},""]
[" -a","厚100mm","m2",225687,null,""]
[" -b","厚100mm（含找平层）","m2",1038287,null,""]
["308-1","透层","m2",1889937,null,""]
["308-2","黏层","m2",2624469,null,""]
["309-2","中粒式沥青混凝土",{"$nulls":3},""]
[" -a","厚50mm","m2",540932,null,""]
["310-2","封层","m2",1889927,null,""]
["311-1","细粒式改性沥青混合料路面",{"$nulls":3},""]
[" -a","厚40mm","m2",1360665,null,""]
["311-2","中粒式改性沥青混合料路面",{"$nulls":3},""]
[" -a","厚50mm","m2",1360290,null,""]
["312-1","水泥混凝土面板",{"$nulls":3},""]
[" -a","厚200mm（混凝土弯拉强度4.5MPa）","m2",128768,null,""]
[" -b","厚280mm（混凝土弯拉强度5.0MPa）","m2",3675,null,""]
[" -c","厚300mm（混凝土弯拉强度5.0MPa）","m2",10175,null,""]
["312-2","钢筋 ",{"$nulls":3},""]
[" -a","光圆钢筋（HPB235、HPB300）","kg",80224,null,""]
[" -b","带肋钢筋（HRB335、HRB400）","kg",7070,null,""]
["312-3","现浇C30混凝土埋板","m3",175,null,""]
["313-1","培路肩",{"$nulls":3},""]
[" -a","培土","m3",67381,null,""]
["313-2","中央分隔带",{"$nulls":3},""]
[" -a","C30混凝土预制板","m3",4542.5,null,""]
[" -b","砂砾垫层","m3",8980,null,""]
[" -c","防渗土工布","m2",149141,null,""]
[" -d","回填土","m3",44100,null,""]
["313-4","混凝土预制块加固路肩",{"$nulls":3},""]
[" -a","C30混凝土","m3",12187.3,null,""]
["313-5","花岗岩条石","m3",5090.4,null,""]
["314-8","过水槽","m",4330,null,""]
["315-1","防裂基布",{"$nulls":3},""]
[" -a","聚丙烯非织造土工布","m2",236940,null,""]
[" -b","普通热沥青粘层油","m2",229887,null,""]
["315-2","路面病害处理",{"$nulls":3},""]
[" -a","热沥青灌缝","m",20333,null,""]
[" -b","回填水泥稳定碎石基层，厚200mm","m2",23925,null,""]
[" -c","回填C30水泥混凝土","m3",898,null,""]
[" -d","碎石土找平，平均厚10cm","m2",249605,null,""]
["清单  第300章合计  人民币(元)",{"$nulls":4},0]

{"sheet":"400章","index":5,"n_rows":125,"n_cols":6,"rows_kept":125,"merged":[[0,0,0,5],[1,0,1,5],[124,0,124,4]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第400章 桥梁、涵洞"]
["合同段编号：ZAZCB",{"$nulls":4},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
["403-1","基础钢筋(包括灌注桩、承台、沉柱、沉井等)",{"$nulls":3},""]
[" -a","光圆钢筋（HPB235、HPB300）","kg",147742.5,null,""]
[" -b","带肋钢筋（HRB335、HRB400）","kg",1091098,null,""]
["403-2","下部结构钢筋",{"$nulls":3},""]
[" -a","光圆钢筋（HPB235、HPB300）","kg",89874.7,null,""]
[" -b","带肋钢筋（HRB335、HRB400）","kg",1135407.7,null,""]
["403-3","上部结构钢筋",{"$nulls":3},""]
[" -a","光圆钢筋（HPB235、HPB300）","kg",965313.6,null,""]
[" -b","带肋钢筋（HRB335、HRB400）","kg",2160819.5,null,""]
["403-4","附属结构钢筋",{"$nulls":3},""]
[" -a","光圆钢筋（HPB235、HPB300）","kg",64791.4,null,""]
[" -b","带肋钢筋(HRB335、HRB400)","kg",1004226.1,null,""]
["404-1","干处挖土方","m3",34214.2,null,""]
["405-1","钻孔灌注桩",{"$nulls":3},""]
[" -a","桩径1.0m","m",743,null,""]
[" -b","桩径1.2m","m",3679,null,""]
[" -c","桩径1.4m","m",72,null,""]
[" -d","桩径1.5m","m",2764,null,""]
[" -e","桩径1.6m","m",140,null,""]
["410-1","混凝土基础（包括支撑梁、桩基承台；但不包括桩基）",{"$nulls":3},""]
[" -a","C15混凝土","m3",59.1,null,""]
[" -b","C20混凝土","m3",68.5,null,""]
[" -c","C25混凝土","m3",42.7,null,""]
[" -d","C25片石混凝土","m3",330.3,null,""]
[" -e","C30混凝土","m3",5173.5,null,""]
["410-2","混凝土下部结构",{"$nulls":3},""]
[" -a","C25混凝土","m3",648.9,null,""]
[" -b","C30混凝土","m3",8596.7,null,""]
[" -c","C35混凝土","m3",1622,null,""]
["410-3","现浇混凝土上部结构",{"$nulls":3},""]
[" -a","C35混凝土","m3",812.2,null,""]
[" -b","C40混凝土","m3",523,null,""]
["410-4","预制混凝土上部结构",{"$nulls":3},""]
[" -a","C50混凝土","m3",1679.5,null,""]
["410-5","上部结构现浇整体化混凝土",{"$nulls":3},""]
[" -a","C40混凝土","m3",40,null,""]
[" -b","C50混凝土","m3",1454.6,null,""]
["410-6","现浇混凝土附属结构",{"$nulls":3},""]
[" -a","C20混凝土","m3",2271.6,null,""]
[" -b","C25片石混凝土","m3",70.6,null,""]
[" -c","C30混凝土","m3",3270.2,null,""]
[" -d","C35混凝土","m3",1939.2,null,""]
[" -e","C40混凝土","m3",38,null,""]
[" -f","C40小石子混凝土","m3",24.2,null,""]
[" -g","C50混凝土","m3",7.4,null,""]
["411-5","后张法预应力钢绞线",{"$nulls":3},""]
[" -a","ΦS15.2","kg",290263.2,null,""]
["411-7","现浇预应力混凝土上部结构",{"$nulls":3},""]
[" -a","C50混凝土箱梁","m3",786.2,null,""]
["411-8","预制预应力混凝土上部结构",{"$nulls":3},""]
[" -a","C50混凝土箱梁","m3",2922.8,null,""]
[" -b","C50混凝土空心板","m3",4719.8,null,""]
["415-2","水泥混凝土桥面铺装",{"$nulls":3},""]
[" -a","C40混凝土，厚100mm","m2",1026,null,""]
[" -b","C50混凝土，厚80mm","m2",3937,null,""]
[" -c","C50混凝土，厚100mm","m2",9337.4,null,""]
[" -d","C50防水混凝土，厚100mm","m2",6956.7,null,""]
[" -e","C50防水混凝土，厚70mm-100mm","m2",136.4,null,""]
[" -f","C50混凝土，厚85mm-160mm","m2",1024.3,null,""]
["415-3","防水层","m2",35610.2,null,""]
["416-1","矩形板式橡胶支座",{"$nulls":3},""]
[" -a","厚10mm","m2",336.3,null,""]
[" -b","GJZ100×200×28","个",4,null,""]
[" -c","GJZ150×200×42","个",16,null,""]
[" -d","GJZ200×300×41","个",2,null,""]
[" -e","GJZ250×300×52","个",36,null,""]
["416-2","圆形板式橡胶支座",{"$nulls":3},""]
[" -a","GYZ200×42","个",816,null,""]
[" -b","GYZ250×52","个",336,null,""]
[" -c","GYZ300×52","个",36,null,""]
[" -d","GYZ450×99","个",164,null,""]
[" -e","GYZF4200×42","个",48,null,""]
[" -f","GYZF4200×44","个",208,null,""]
[" -g","GYZF4250×43","个",96,null,""]
[" -h","GYZF4450×101","个",72,null,""]
["416-4","盆式支座",{"$nulls":3},""]
[" -a","GPZ2.5DX","个",2,null,""]
[" -b","GPZ2.5SX","个",2,null,""]
[" -c","GPZ3.5DX","个",4,null,""]
[" -d","GPZ3.5SX","个",2,null,""]
[" -e","GPZ3.5GD","个",2,null,""]
[" -f","GPZ5.0DX","个",1,null,""]
[" -g","GPZ5.0GD","个",1,null,""]
["417-2","模数式伸缩装置",{"$nulls":3},""]
[" -a","40型","m",251.3,null,""]
[" -b","80型","m",492,null,""]
["419-1","单孔钢筋混凝土圆管涵",{"$nulls":3},""]
[" -a","φ0.75m","m",792,null,""]
[" -b","φ1.0m","m",332,null,""]
["420-1","钢筋混凝土盖板涵",{"$nulls":3},""]
[" -a","1-2.0m×净高1.0m","m",70,null,""]
[" -b","1-2.0m×净高1.5m","m",952.3,null,""]
[" -c","1-2m×净高1.5m（利用）","m",55.48,null,""]
[" -d","1-2.0m×净高2.0m","m",43,null,""]
[" -e","1-2.0m×净高2.0m（利用）","m",1,null,""]
[" -f","1-3.5m×净高2.2m","m",10,null,""]
[" -g","1-3.5m×净高2.5m","m",12.53,null,""]
[" -h","1-3.5m×净高2.5m（利用）","m",3,null,""]
[" -i","1-4.0m×净高1.5m","m",95.8,null,""]
[" -j","1-4.0m×净高2.0m","m",179.08,null,""]
[" -k","1-4.0m×净高2.5m","m",6.9,null,""]
[" -l","1-4.0m×净高2.75m（利用）","m",9,null,""]
[" -m","1-4.0m×净高3.0m","m",38.5,null,""]
[" -m","1-4.0m×净高3.5m（利用）","m",20,null,""]
[" -n","2-6.0m×净高2.5m","m",24,null,""]
[" -o","2-6.0m×净高3.5m","m",52,null,""]
["422-1","加固维修",{"$nulls":3},""]
[" -a","裂缝封闭","m",125,null,""]
[" -b","铰缝修补及勾缝2cm","m2",230.7,null,""]
[" -c","上部混凝土缺陷修复","m2",19.4,null,""]
[" -d","墩台混凝土缺陷修复","m2",18.8,null,""]
[" -e","洞身混凝土缺陷修复","m2",18,null,""]
[" -f","锥坡修复","m2",821,null,""]
[" -g","锥坡灌浆","m",600,null,""]
[" -h","C20混凝土帽石","m3",10.1,null,""]
[" -i","C20片石混凝土涵底、洞口及沟渠","m3",1135.9,null,""]
[" -j","M7.5浆砌八字墙","m3",7.4,null,""]
[" -k","植筋(HRB335、HRB400)","kg",14767.4,null,""]
[" -l","伸缩缝更换","m",450,null,""]
[{"$nulls":5},""]
["清单  第400章合计  人民币(元)",{"$nulls":4},0]

{"sheet":"600章","index":6,"n_rows":96,"n_cols":6,"rows_kept":96,"merged":[[0,0,0,5],[1,0,1,5],[95,0,95,4]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第600章 安全设施"]
["合同段编号：ZAZCB",{"$nulls":4},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
["602-2","路侧护栏",{"$nulls":3},""]
[" -a","AT1","m",972,null,""]
[" -b","AT2","m",1020,null,""]
[" -c","BT-1","m",2970,null,""]
[" -d","BT-2","m",66,null,""]
[" -e","DT","m",464,null,""]
[" -f","Gr-A-4E","m",110498,null,""]
[" -g","Gr-A-2E","m",22992,null,""]
[" -h","Gr-SB-2E","m",1853,null,""]
["602-3","中央分隔带护栏",{"$nulls":3},""]
[" -a","Gr-Am-4E","m",104514,null,""]
[" -b","Grd-Am-2E","m",2939,null,""]
[" -c","Gr-SBm-2E","m",1040,null,""]
[" -d","CT","m",1680,null,""]
[" -e","CT1","m",45,null,""]
[" -f","推拉式活动护栏","m",390,null,""]
[" -g","活动护栏","m",1040,null,""]
[" -h","匝道中分带混凝土护栏","m",271,null,""]
["603-2","刺钢丝隔离栅",{"$nulls":3},""]
[" -a","F-Bw-C","m",105578,null,""]
["603-4","电焊网隔离栅",{"$nulls":3},""]
[" -a","F-Ww-C","m",20494,null,""]
["603-5","桥梁防抛网",{"$nulls":3},""]
[" -a","Bf-Ww-B","m",3080,null,""]
["604-1","单柱式交通标志",{"$nulls":3},""]
[" -a","△900","个",113,null,""]
[" -b","2-△900","个",8,null,""]
[" -c","△1300","个",18,null,""]
[" -d","□1100×2300","个",10,null,""]
[" -e","□1200×900+Φ1200","个",42,null,""]
[" -f","□1700×1200+□1800×660","个",7,null,""]
[" -g","2-□400×400","个",16,null,""]
[" -h","2-□400×600","个",54,null,""]
[" -i","2-□600×800","个",31,null,""]
[" -j","六边形700×480","个",54,null,""]
[" -k","□2000×1000","个",22,null,""]
[" -l","□2000×3000","个",6,null,""]
[" -m","□900×3200","个",19,null,""]
[" -n","八边形800","个",4,null,""]
[" -o","□600×800","个",703,null,""]
[" -p","Φ800","个",32,null,""]
[" -q","Φ800+△900","个",21,null,""]
[" -r","Φ1200","个",24,null,""]
[" -s","□1200×900+2-Φ1200","个",24,null,""]
["604-2","双柱式交通标志",{"$nulls":3},""]
[" -a","□3200×2900","个",5,null,""]
[" -b","□4200×3200","个",19,null,""]
[" -c","□5200×3100","个",17,null,""]
[" -d","□5200×3600","个",7,null,""]
[" -e","□5700×3800","个",9,null,""]
[" -f","□5700×3800+□2350×1000","个",6,null,""]
[" -g","□6000×5550","个",2,null,""]
["604-4","门架式交通标志",{"$nulls":3},""]
[" -a","3-□2900×3600+2-□1400×3200","个",8,null,""]
[" -b","□3500×3800+□5700×3800+□2350×1000","个",6,null,""]
["604-5","单悬臂式交通标志",{"$nulls":3},""]
[" -a","□3000×2800","个",10,null,""]
[" -b","□3400×3900","个",8,null,""]
[" -c","□3800×1800","个",4,null,""]
[" -d","□4200×3200","个",12,null,""]
[" -e","□5200×3100","个",1,null,""]
[" -f","□5400×5000","个",6,null,""]
[" -g","□5700×3800+□2350×1000","个",2,null,""]
["604-6","双悬臂式交通标志",{"$nulls":3},""]
[" -a","2-□3400×3200+□2350×1000","个",6,null,""]
[" -b","2-□3700×1800","个",3,null,""]
["604-7","附着式交通标志",{"$nulls":3},""]
[" -a","Φ100","个",986,null,""]
[" -b","Φ1000","个",26,null,""]
[" -c","□400×400","个",19,null,""]
[" -d","□520×320","个",50,null,""]
[" -e","□1500×700","个",10,null,""]
["604-8","里程碑","个",63,null,""]
["604-9","公路界碑","个",973,null,""]
["604-10","百米桩","个",572,null,""]
["605-1","路面标线",{"$nulls":3},""]
[" -a","热熔标线","m2",104517,null,""]
[" -b","减速标线","m2",2590,null,""]
[" -c","视觉减速标线","m2",2895,null,""]
["605-6","轮廓标",{"$nulls":3},""]
[" -a","De-Rbw-At1","个",16481,null,""]
[" -b","De-Rbw-At2","个",246,null,""]
[" -c","De-Rbw-E","个",499,null,""]
[" -d","De-Rby-At1","个",6050,null,""]
[" -e","De-Rby-At2","个",170,null,""]
["605-7","立面标记","m2",95,null,""]
["606-2","防眩网",{"$nulls":3},""]
[" -a","Gs-N-C","m",58698,null,""]
[" -b","Gs-N-Gw","m",1196,null,""]
[{"$nulls":5},""]
[{"$nulls":5},""]
["清单  第600章合计  人民币(元)",{"$nulls":4},0]

{"sheet":"700章","index":7,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[1,0,1,5],[22,0,22,4]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第700章 绿化及环境保护设施"]
["合同段编号：ZAZCB",{"$nulls":4},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
["703-1","撒播草种","m2",85924,null,""]
["704-1","人工种植乔木",{"$nulls":3},""]
[" -a","金叶榆（胸径3-4cm）","株",12,null,""]
[" -b","东北云杉（苗高2.0-2.5m，冠径1.5m）","株",234,null,""]
[" -c","樟子松（苗高2.5-3.0m，冠径1.8m）","株",357,null,""]
[" -d","五角枫（胸径5-6cm）","株",232,null,""]
[" -e","旱柳（胸径5-6cm）","株",17,null,""]
[" -f","桧柏（冠径0.3m，高度1m）","株",5300,null,""]
["704-2","人工种植灌木",{"$nulls":3},""]
[" -a","石竹","株",4643,null,""]
[" -b","榆叶梅（苗高1.2m，7-10分枝/株）","株",120,null,""]
[" -c","黄刺玫（苗高1.2m，7-10分枝/株）","株",220,null,""]
[" -d","丁香（苗高1.2m，7-10分枝/株）","株",670,null,""]
[" -e","萱草","株",2085,null,""]
["706-1","声屏障",{"$nulls":3},""]
[" -a","路基段声屏障","m",3772,null,""]
[" -b","桥梁段声屏障","m",123,null,""]
[{"$nulls":5},""]
["清单  第700章合计  人民币(元)",{"$nulls":4},0]

{"sheet":"800章","index":8,"n_rows":40,"n_cols":6,"rows_kept":40,"merged":[[0,0,0,5],[1,0,1,5],[39,0,39,4]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第800章 房建工程"]
["合同段编号：ZAZCB",{"$nulls":4},"货币单位：人民币元"]
["子目号","子  目  名  称","单 位","数 量","单价","合价"]
[801,"大河湾收费站"]
[{"v":1,"d":"-1"},"收费站综合楼","m2",1185.2,null,""]
[{"v":2,"d":"-2"},"收费站车库","m2",222.84,null,""]
[{"v":3,"d":"-3"},"养护工区综合楼","m2",1185.2,null,""]
[{"v":4,"d":"-4"},"养护车库","m2",446.76,null,""]
[{"v":5,"d":"-5"},"水泵房","m2",177.66,null,""]
[{"v":6,"d":"-6"},"柴油发电机房","m2",57.51,null,""]
[{"v":7,"d":"-7"},"消防水池","座",1,null,""]
[{"v":8,"d":"-8"},"取水井","座",2,null,""]
[{"v":9,"d":"-9"},"铁艺围墙","m",880,null,""]
[{"v":10,"d":"-10"},"道路广场及停车场","m2",13505.5,null,""]
[{"v":11,"d":"-11"},"绿化工程","m2",15585.96,null,""]
[{"v":12,"d":"-12"},"其他工程","项",1,null,""]
[802,"音河服务区",{"$nulls":3},""]
[{"v":1,"d":"-1"},"服务区综合楼","m2",4460.26,null,""]
[{"v":2,"d":"-2"},"维修车间","m2",452.4,null,""]
[{"v":3,"d":"-3"},"水泵房","m2",344.72,null,""]
[{"v":4,"d":"-4"},"柴油发电机房","m2",115.2,null,""]
[{"v":5,"d":"-5"},"加油站","m2",263.9,null,""]
[{"v":6,"d":"-6"},"消防水池","座",2,null,""]
[{"v":7,"d":"-7"},"取水井","座",2,null,""]
[{"v":8,"d":"-8"},"围墙","m",973.71,null,""]
[{"v":9,"d":"-9"},"道路广场及停车场","m2",45200.52,null,""]
[{"v":10,"d":"-10"},"绿化工程","m2",14215.16,null,""]
[{"v":11,"d":"-11"},"其他工程","项",1,null,""]
[803,"向阳峪停车区",{"$nulls":3},""]
[{"v":1,"d":"-1"},"服务区综合楼","m2",377.4,null,""]
[{"v":2,"d":"-2"},"取水井","座",2,null,""]
[{"v":3,"d":"-3"},"铁艺围墙","m",524.23,null,""]
[{"v":4,"d":"-4"},"道路广场及停车场","m2",14881.8,null,""]
[{"v":5,"d":"-5"},"绿化工程","m2",4250.66,null,""]
[{"v":6,"d":"-6"},"其他工程","项",1,null,""]
[804,"阿荣旗南收费站",{"$nulls":3},""]
[{"v":1,"d":"-1"},"UPS电源室","m2",57.51,null,""]
[{"v":2,"d":"-2"},"维修费用","项",1,null,""]
["清单 第800章合计  人民币(元) ",{"$nulls":4},0]

{"sheet":"900章","index":9,"n_rows":351,"n_cols":8,"rows_kept":351,"merged":[[0,0,0,7],[1,0,1,7],[33,7,36,7],[350,0,350,5]],"flags":["formulas_cached_only"]}
["工程量清单"]
["清单  第900章 机电工程"]
["合同段编号：ZAZCB",{"$nulls":6},"货币单位：人民币元"]
["子目号","子  目  名  称","规格","单位","数量","单价","合价","备注"]
["900-1","监控系统",{"$nulls":4},""]
["900-1-2","交通调查站",{"$nulls":4},""]
[-1,"一类交通调查站（基础、机箱、防雷器、接地工程、附件及完成本系统所需的其他材料及工作）","线圈加压电感式交通量调查站，含软件","套",1,null,""]
[-2,"二类交通调查站（含立柱、基础、机箱、防雷器、接地工程、附件及完成本系统所需的其他材料及工作）","微波，含软件","套",2,null,""]
["900-1-3","可变信息标志",{"$nulls":4},""]
[-1,"悬臂式可变信息标志显示屏（含立柱、基础、机箱、防雷器、接地工程、附件及完成本系统所需的其他材料及工作）","显示板面: 3.2m×1.6m；双基色显示；节能型","套",3,null,""]
[-2,"门架式可变信息标志显示屏（含门架、基础、机箱、防雷器、接地工程、附件及完成本系统所需的其他材料及工作）","信息显示屏：10m×1m；1块全彩色，9块双基色；节能型","套",2,null,""]
[-3,"服务区信息发布屏(含门架、基础、机箱、防雷器、接地工程、附件及完成本系统所需的其他材料及工作)","显示板面: 4m×3m；发光二极管（LED）构成显示像素\n","套",2,null,""]
["900-1-4","闭路电视系统",{"$nulls":4},""]
[-1,"枪式遥控高清摄像机（含立柱、基础、机箱、避雷针、防雷器、接地工程、安装附件等）","含云台，防护罩","套",6,null,""]
[-2,"彩色球形摄像机（含立柱、基础、机箱、避雷针、防雷器、接地工程、安装附件等）","高清显示","台",6,null,""]
[-3,"视频存储阵列","含硬盘","套",1,null,""]
[-4,"视频管理工作站",null,"台",1,null,""]
[-5,"支线传输电缆","视频电缆及信号电缆","项",1,null,""]
[-6,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-1-5","气象检测器",{"$nulls":4},""]
[-1,"气象检测器（含立柱、基础、机箱、防雷器、接地工程、附件及完成本系统所需的其他材料及工作）","温度、湿度、能见度、风速、风向、道面结冰","套",1,null,""]
["900-1-6","信息传输",{"$nulls":4},""]
[-1,"以太网数据光端机",null,"台",7,null,"","收费站机房"]
[-2,"视频数据复用光端机",null,"台",29,null,""]
[-3,"数据以太网交换机",null,"对",11,null,""]
[-4,"视频以太网交换机（服务区内）",null,"对",16,null,""]
[-5,"视频编码器",null,"个",126,null,""]
[-6,"单模光缆","GYTA-4B1","千米",6,null,""]
[-7,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
[-8,"上级分中心监控软件升级",null,"项",1,null,""]
["900-1-7","外场设备供电",{"$nulls":4},""]
[-1,"室内配电箱（含断路器）",null,"套",2,null,""]
[-2,"室外监控配电箱（含断路器）","室外型、含基础","套",5,null,""]
[-3,"电力电缆",{"$nulls":4},"","具体的数量以工程实际数量为准，但投标书中以本招标文件报价"]
[-3.1,"电力电缆YJV22-4×16",null,"千米",2.5,null,""]
[-3.2,"电力电缆YJV22-4×10",null,"千米",3.05,null,""]
[-3.3,"电力电缆YJV22-2×6",null,"千米",2.02,null,""]
[-4,"风光互补供电设备",null,"套",4,null,""]
[-5,"手孔",null,"个",23,null,""]
[-6,"边坡修复","敷设电缆","项",1,null,""]
[-7,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-1-8","监控外场设备防雷保护",{"$nulls":4},""]
[-1,"SPD1三相B、C级电源防雷器",null,"套",2,null,""]
[-2,"SPD2单相B、C级电源防雷器",null,"套",21,null,""]
[-3,"SPD5 视频信号防雷器",null,"只",12,null,""]
[-4,"SPD6 数据信号防雷器",null,"只",23,null,""]
[-5,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-1-9","监控外场设备基础及接地",{"$nulls":4},""]
[-1,"遥控摄像机基础及接地（变电所供电）",null,"套",2,null,""]
[-2,"遥控摄像机基础及接地（变电所供电）",null,"套",4,null,""]
[-3,"球形摄像机基础及接地",null,"套",6,null,""]
[-4,"门架式可变信息标志基础及接地",null,"套",2,null,""]
[-5,"悬臂式可变信息标志基础及接地",null,"套",3,null,""]
[-6,"服务区信息发布屏基础及接地",null,"套",2,null,""]
[-7,"气象检测器基础及接地",null,"套",1,null,""]
[-8,"一类交通调查站基础及接地",null,"套",1,null,""]
[-9,"二类交通调查站基础及接地",null,"套",2,null,""]
[-10,"室外配电箱基础及接地",null,"套",5,null,""]
["900-1-14","备件、随机备件和专用工具",{"$nulls":4},""]
[-1,"视频数据复用光端机","单模光纤","套",1,null,""]
[-2,"数据光端机","单模光纤","套",1,null,""]
[-3,"视频编码器",null,"套",1,null,""]
[-4,"遥控摄像机",null,"套",1,null,""]
[-5,"可变信息标志驱动电路板",null,"块",2,null,""]
[-6,"万用表",null,"套",1,null,""]
[-7,"网络通断测试仪",null,"套",1,null,""]
[-8,"维修组合工具",null,"套",1,null,""]
[-9,"地阻表",null,"套",1,null,""]
["900-2","通信系统",{"$nulls":4},""]
["900-2-2","光纤传输工程",{"$nulls":4},""]
["-1","干线联合调试","东部区域中心、阿荣旗分中心、呼伦贝尔分中心干线联合调试，以及由于本项目的接入对相关路段进行的所有调试及扩容","项",1,null,""]
[-2,"*综合光接入网局端设备(OLT)扩容","OLT设备STM-4等级光接口2个、V5.2接口2个，以太网接口4个及辅材，并将新增站点接入该OLT设备，并调通。","套",1,null,"","阿荣旗分中心"]
[-3,"*综合光接入网远端设备(ONU)","内置2块STM-4等级（622Mbit/s）光接口板,至少8路10/100M以太网接口，至少2路1000M以太网接口，至少16路E1接口，含设备机柜、标准机架、电源、公共单元及相应辅材等。","套",2,null,"","大河湾收费站、音河服务区"]
[-4,"传输网管、接入网管系统调试",null,"项",1,null,""]
[-5,"*便携式网管（含软件及设备）","网管系统应高于以下配置：处理器： 酷睿i5 2代系列，CPU频率：2400MHz 或以上；\n内存DDR3 1333MHz 4G；\n硬盘≥500GB；操作系统：Win 7 专业版或以上版本；光驱类型：DVD刻录机","套",1,null,""]
[-6,"*电话光端机","光接口：比特率：155.52Mb/s，波长1310nm至少30路音频接口，至少2路10M/ 100M的以太网接口；","对",1,null,"","服务区"]
[-7,"*电话光端机","光接口：比特率：155.52Mb/s，波长1310nm至少16路音频接口；至少2路10M/ 100M的以太网接口；","对",2,null,"","停车区"]
[-8,"*综合配线柜（DDF、ODF）","配置光纤配线单元≥120芯、数字配线单元≥16系统、以太网配线单元≥24线，含机柜等辅材","套",3,null,"","阿荣旗分中心、大河湾收费站、音河服务区"]
[-9,"*MDF保安配线柜","含200回线配线单元","套",3,null,"","阿荣旗分中心、大河湾收费站、音河服务区"]
[-10,"综合配线箱","光纤配线单元≥36芯线， 音频配线单元≥100线，含及机柜等辅材","套",3,null,"","服务区、停车区"]
[-11,"安装材料及连接装置、电缆、设备底座（有人、无人通信站）",null,"站区",3,null,""]
[-12,"安装材料及连接装置、电缆、设备底座（服务区、停车区）",null,"站区",1,null,""]
["-13","安装材料及连接装置、电缆（电话光端机）",null,"套",3,null,""]
["-14","打印机","激光打印，A3\\A4幅面","台",1,null,""]
["900-2-3","光缆线路工程",{"$nulls":4},""]
[-1,"*24芯单模层绞式光缆","GYTA单模光缆","km",131.6,null,"","据实计量"]
[-2,"*4芯单模层绞式光缆","GYTA单模光缆","km",5,null,"","据实计量"]
[-3,"3孔LDPE子管","φ32/26","延米",2000,null,"","据实计量"]
[-4,"光缆接头盒",null,"个",70,null,""]
[-5,"光缆终端盒",null,"个",4,null,""]
[-6,"光缆接续材料及光缆跳接熔接","含尾纤、跳线等所有接续材料","项",4,null,""]
[-7,"市话电缆","HYTA-30*2*0.5","米",2900,null,"","据实计量"]
[-8,"线路防雷装置",null,"项",4,null,""]
["900-2-4","程控交换系统",{"$nulls":4},""]
[-1,"*数字程控交换机扩容及调试","含2块2M数字中继板、2块主节点板及辅材，新增2个V5.2接口及100线本地语音接入","项",1,null,""]
[-2,"按钮电话机","DTMF","部",153,null,""]
[-3,"传真机","G3","台",7,null,""]
[-4,"安装材料",null,"项",4,null,""]
["900-2-5","通信电源工程",{"$nulls":4},""]
["-1","交流配电柜",null,"套",2,null,""]
["-2","*48V/3×10A高频开关型组合电源","①输入电压：AC220V，频率50 HZ±5%范围内正常运行；输出：DC-48V，输出电压允许值-43～-56V，功率因数：COSΦ≥0.9，定电压：DC-48V。\n②杂音电压：≤2mV衡重杂音、动电压：≤200mV（P～P值）、效率：≥90%\n③输出路数：满足输出电路数量和容量要求，并留有余量，可接入两组蓄电池，控制蓄电池组的过充电、过放电。","套",2,null,"","带监控模块"]
[-3,"阀控式密封蓄电池","–48V、100Ah","组",4,null,""]
[-4,"*UPS电源","220V、2kVA","套",3,null,"","服务区、停车区"]
[-5,"电力电缆","VV22-4×16+1×10","米",400,null,"","据实计量"]
[-6,"电力电缆","VV-1×35","米",80,null,"","据实计量"]
[-7,"电力电缆","VV-1×10","米",100,null,"","据实计量"]
[-8,"接地总汇集铜排","550×80×8铜排","块",2,null,""]
[-9,"通信接地汇流排","550×80×8铜排","块",2,null,""]
[-10,"接地引线","BV-1×50","米",360,null,""]
[-11,"接地引线","BV-1×35","米",100,null,""]
[-12,"电缆桥架300×150×2000mm",null,"m",100,null,"","据实计量"]
[-13,"防静电地板下200×100金属走线槽",null,"m",100,null,"","据实计量"]
[-14,"系统接地",null,"项",1,null,""]
[-14,"辅助材料","含抗震底座、供电及配套电缆、防雷接地等","项",4,null,""]
["900-2-10","备件、随机备件和专用工具",{"$nulls":4},""]
[-1,"STM-4光接口板",null,"块",1,null,""]
[-2,"以太网板",null,"块",1,null,""]
[-3,"模拟用户板",null,"块",1,null,""]
[-4,"电源板",null,"块",1,null,""]
[-5,"单模尾纤",null,"根",30,null,""]
[-6,"单模光纤跳线",null,"根",30,null,""]
[-7,"5类非屏蔽双绞线",null,"米",100,null,""]
[-8,"RJ45接头",null,"个",30,null,""]
[-9,"压线钳",null,"把",2,null,""]
[-10,"卡线钳",null,"把",2,null,""]
[-11,"万用表",null,"台",2,null,""]
[-12,"2M误码仪",null,"台",1,null,""]
[-13,"网线通断测试仪",null,"个",2,null,""]
[-14,"接地电阻测试仪",null,"台",1,null,""]
[-15,"小型组合工具箱",null,"套",1,null,""]
["900-3","收费系统",{"$nulls":4},""]
["900-3-2","收费软件",{"$nulls":4},""]
[-1,"收费站服务器操作系统软件",null,"套",2,null,""]
[-2,"收费站数据库管理软件",null,"套",2,null,""]
[-3,"收费站工作站操作系统软件",null,"套",8,null,""]
[-4,"收费车道操作系统软件",null,"套",22,null,""]
[-5,"MTC收费站应用软件","采用自治区联网收费统一软件","套",2,null,""]
[-6,"ETC收费站应用软件","采用自治区联网收费统一软件","套",2,null,""]
[-7,"MTC收费车道应用软件","采用自治区联网收费统一软件","套",16,null,""]
[-8,"ETC收费车道应用软件","采用自治区联网收费统一软件","套",6,null,""]
[-9,"杀毒软件（网络版）","采用正版的具有许可证的软件","套",2,null,""]
[-10,"网络通信软件",null,"套",2,null,""]
[-11,"中间件软件","采用正版的具有许可证的软件","套",2,null,""]
[-12,"上级分中心收费软件升级",null,"项",1,null,""]
["900-3-3","收费站设备",{"$nulls":4},""]
[-1,"容错服务器",null,"台",2,null,""]
[-2,"管理工作站","CPU：酷睿i7六核，主频≥3.4GHz，内存8G，硬盘1TG，独立显卡1G，22”液晶显示器，100M以太网卡","台",6,null,""]
[-3,"三层以太网交换机","三层千兆交换机， 24口10/100M/1000M路由交换机，2个1000M单模光口","台",2,null,""]
[-4,"激光黑白打印机","A3/A4，支持网络打印","台",2,null,""]
[-5,"彩色激光打印机","A3/A4，支持网络打印","台",2,null,""]
[-6,"针式打印机",null,"台",2,null,""]
[-7,"光盘刻录机",null,"台",2,null,""]
[-8,"移动硬盘","2TB","台",2,null,""]
[-9,"非接触IC卡读写器","非接触","台",2,null,"","采用自治区联网收费统一的IC卡读写器"]
[-10,"报警主机","16个开关量报警输入","台",2,null,""]
[-11,"对讲主机","带录音按钮电话，全双工通信方式","台",2,null,""]
[-12,"设备机柜","19寸标准机柜","台",4,null,""]
[-13,"收费机房综合操作台","含座椅","台",2,null,""]
[-14,"财务室桌椅",null,"套",2,null,""]
[-15,"电子投包机","由库体、电脑控制及网络系统构成","台",2,null,""]
[-16,"收费机房金属线槽",null,"项",1,null,""]
[-17,"非接触IC卡",null,"张",56000,null,""]
[-18,"16路语音光端机",null,"对",2,null,""]
[-19,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-3-4","MTC收费车道设备",{"$nulls":4},""]
[-1,"车道收费机（含车道工控机、车道控制器）","工业级CPU主板，主频2.0GHz以上，1G以上具有奇偶检验功能内存，160G SATAⅡ硬盘，I/O控制卡和多串口卡，100M网卡","台",16,null,""]
[-2,"专用键盘","内蒙古自治区统一键盘","台",16,null,"","采用自治区联网收费统一的专用键盘"]
[-3,"显示器","19″液晶显示器","台",16,null,""]
[-4,"视频捕捉卡",null,"台",16,null,""]
[-5,"车检检测器","双通道","台",16,null,""]
[-6,"票据打印机",null,"台",11,null,"","票据打印机应适应自治区联网收费技术要求"]
[-7,"自动栏杆",null,"台",16,null,""]
[-8,"手动栏杆","栏杆臂采用不锈钢材料","台",16,null,""]
[-9,"非接触IC卡读写器","非接","台",16,null,"","采用自治区联网收费统一的IC卡读写器"]
[-10,"便携式车道收费机","包括主机、液晶显示屏、专用键盘、IC卡读写器、备用电源","台",4,null,""]
[-11,"IC卡卡箱",null,"台",80,null,""]
[-12,"车牌识别器（含软件）",null,"套",16,null,""]
[-13,"天棚信号灯","LED，红色“×”绿色“↓”","套",16,null,""]
[-14,"雾灯","采用超高亮黄色LED组成，包含立柱及法兰","台",16,null,""]
[-15,"车道通行信号灯(含闪光报警器)","LED，包含立柱及法兰盘","台",5,null,""]
[-16,"费额显示器（含信号灯、报警器）","费额显示器由19位超高亮度红色LED七段数码构成，包含立柱及法兰盘","套",11,null,"","采用全省联网收费统一的费额显示模式"]
[-17,"对讲电话","普通按钮电话，全双工通信方式","台",16,null,""]
[-18,"安全报警开关",null,"台",16,null,""]
[-19,"车道设备机柜","标准机柜，容量为16U","台",2,null,""]
[-20,"广场以太网交换机","快速二层交换机，12个10/100M/1000M电口，≥2个100M/1000M光口；","台",4,null,""]
[-21,"收费员操作台（含座椅）",null,"台",16,null,""]
[-22,"收费亭空调",null,"套",16,null,""]
[-23,"超宽车道计重设备","（含双承台秤、红外光栅车辆分割器、检测线圈、胎型识别器室外机箱、软件、设备基础等）","套",2,null,""]
[-24,"普通车道计重设备","（含双承台秤、红外光栅车辆分割器、检测线圈、胎型识别器室外机箱、软件、设备基础等）","套",9,null,""]
[-25,"衡器鉴定费",null,"套",11,null,""]
[-26,"窗口对讲机",null,"台",16,null,""]
[-27,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-3-5","ETC收费车道设备",{"$nulls":4},""]
[-1,"车道收费机（含车道工控机、车道控制器）","工业级CPU主板，主频2.0GHz以上，1G以上具有奇偶检验功能内存，160G SATAⅡ硬盘，I/O控制卡和多串口卡，100M网卡","台",6,null,""]
[-2,"显示器","19″液晶显示器","台",6,null,""]
[-3,"专用键盘","内蒙自治区统一键盘","台",6,null,"","采用自治区联网收费统一的专用键盘"]
[-4,"ETC专用车辆检测器",null,"套",6,null,""]
[-5,"路侧读写单元(含双天线)","含2个天线和2个天线控制器，ETC双天线立柱及支架","套",6,null,"","含2个天线和2个天线控制器"]
[-6,"高速自动栏杆","栏杆起落时间小于0.7秒，具有智能防砸车功能","套",6,null,""]
[-7,"ETC专用费额显示器","费额显示器采用红、绿双基色表贴LED显示，包含立柱及法兰盘","套",6,null,""]
[-8,"车牌识别器（含软件）",null,"套",6,null,""]
[-9,"天棚信号灯","LED，红色“×”绿色“↓”","套",6,null,""]
[-10,"雾灯","采用超高亮黄色LED组成，包含立柱及法兰","台",6,null,""]
[-11,"对讲电话","普通按钮电话，全双工通信方式","台",6,null,""]
[-12,"检测线圈",null,"套",6,null,""]
[-13,"收费亭配电箱","含箱体、开关、熔断器等","个",6,null,""]
[-14,"收费员操作台（含座椅）",null,"台",6,null,""]
[-15,"收费亭空调",null,"套",6,null,""]
[-16,"车道LED显示屏及门架","显示面积3200mm×640mm，双基色显示","套",6,null,""]
[-17,"收费员操作台（含座椅）",null,"台",6,null,""]
[-18,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-3-6","闭路电视监视系统",{"$nulls":4},""]
[-1,"亭内拾音器",null,"台",22,null,""]
[-2,"收费亭摄像机",null,"套",22,null,""]
[-3,"车道摄像机",null,"套",22,null,""]
[-4,"收费广场摄像机","含立柱、基础、避雷针、接地、设备箱","套",4,null,""]
[-5,"财务室摄像机",null,"套",2,null,""]
[-6,"监控室摄像机",null,"套",2,null,""]
[-7,"2路视频远端模块",null,"台",24,null,""]
[-8,"单路视频远端模块",null,"对",4,null,""]
[-9,"4路视频解码器",null,"台",11,null,""]
[-10,"视频以太网交换机","三层千兆交换机， 24口10/100M/1000M路由交换机，2个1000M单模光口","台",2,null,""]
[-11,"IP-san磁盘阵列","IP SAN网络存储，RAID支持：RAID 0,1,3,5,6,10,50","台",2,null,""]
[-12,"视频存储服务器",null,"台",2,null,""]
[-13,"图形管理工作站",null,"台",2,null,""]
[-14,"监视器墙",null,"套",2,null,""]
[-15,"32\"液晶监视器",null,"台",44,null,""]
[-16,"32\"主监视器",null,"台",2,null,""]
[-17,"主控键盘",null,"套",2,null,""]
[-18,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-3-7","电源及防雷系统",{"$nulls":4},""]
[-1,"UPS模块(15KVA)","含UPS电池组","台",6,null,""]
[-2,"监控室配电箱",null,"台",4,null,""]
[-3,"广场配电箱",null,"台",2,null,""]
[-4,"稳压电源",null,"台",2,null,""]
[-5,"电源防雷",null,"项",1,null,""]
[-6,"网络避雷",null,"项",1,null,""]
[-7,"视频防雷",null,"项",1,null,""]
[-8,"收费站机房及广场接地","含接地铜排等接地设备","项",1,null,""]
[-9,"完成本系统所需的其他材料及工作",null,"项",1,null,""]
["900-3-8","线缆及光缆",{"$nulls":4},""]
[-1,"单模光缆（4芯）",null,"m",2800,null,"","具体的数量以工程实施数量为准"]
[-2,"单模光缆（10芯）",null,"m",2800,null,"","具体的数量以工程实施数量为准"]
[-3,"网络电缆（UTP-5）",null,"m",1000,null,"","具体的数量以工程实施数量为准"]
[-4,"视频电缆",null,"m",1500,null,"","具体的数量以工程实施数量为准"]
[-5,"电力电缆 YJV-1.0/0.6KV-5*35",null,"m",1000,null,"","具体的数量以工程实施数量为准"]
[-6,"电力电缆 YJV-1.0/0.6KV-3*16",null,"m",1500,null,"","具体的数量以工程实施数量为准"]
[-7,"电力电缆ZR-BVV-0.6/1KV 3×4 ",null,"m",1100,null,"","具体的数量以工程实施数量为准"]
[-8,"电力电缆（RVV-3X2.5）",null,"m",400,null,"","具体的数量以工程实施数量为准"]
[-9,"电力电缆（WDZ-VV4*1.5）",null,"m",3600,null,"","具体的数量以工程实施数量为准"]
[-10,"电力电缆（WDZ-VV3*1.5）",null,"m",4400,null,"","具体的数量以工程实施数量为准"]
[-11,"电力电缆（WDZ-VV2*1.5）",null,"m",500,null,"","具体的数量以工程实施数量为准"]
[-12,"电力电缆（WDZ-RVV10*1.5）",null,"m",500,null,"","具体的数量以工程实施数量为准"]
[-13,"信号电缆（RVV 3×0.5）",null,"m",500,null,"","具体的数量以工程实施数量为准"]
[-14,"信号电缆（RVV 2×0.5）",null,"m",1100,null,"","具体的数量以工程实施数量为准"]
["900-3-8","收费土建",{"$nulls":4},""]
[-1,"28m单向收费岛",null,"个",5,null,""]
[-2,"34m单向收费岛",null,"个",1,null,""]
[-3,"40m单向收费岛",null,"个",11,null,""]
[-4,"46m单向收费岛",null,"个",1,null,""]
[-5,"60m双向收费岛",null,"个",2,null,""]
[-6,"路肩人孔",null,"个",8,null,""]
[-7,"供电手孔",null,"个",4,null,""]
[-8,"收费岛上手孔",null,"个",40,null,""]
[-9,"单向收费亭",null,"个",18,null,""]
[-10,"双向收费亭",null,"个",2,null,""]
[-11,"预埋钢管","φ114×4.0mm钢管","米",2000,null,"","收费广场横穿管"]
[-12,"预埋钢管","φ60×3.5mm钢管","米 ",3200,null,"","岛内设备、边坡预埋管(不含进入天棚手孔管道)"]
[-13,"雾灯基础","含法兰盘、地脚螺栓","个",22,null,""]
[-14,"手动栏杆基础","含法兰盘、地脚螺栓","个",22,null,""]
[-15,"费额显示器基础","含法兰盘、地脚螺栓","个",17,null,""]
[-16,"天棚立柱手孔",null,"个",16,null,""]
[-17,"称重控制箱基础","含法兰盘、地脚螺栓","个",11,null,""]
[-18,"自动栏杆基础","含法兰盘、地脚螺栓","个",22,null,""]
[-19,"通行信号灯基础","含法兰盘、地脚螺栓","个",5,null,""]
[-20,"ETC天线基础","含法兰盘、地脚螺栓","个",6,null,""]
[-21,"ETC车道LED显示屏基础","含法兰盘、地脚螺栓",null,6,null,""]
[-22,"车道摄像机基础","含法兰盘、地脚螺栓","个",22,null,""]
[-23,"广场摄像机基础","含法兰盘、地脚螺栓","个",4,null,""]
["900-3-9","测试仪表及专用工具",{"$nulls":4},""]
[-1,"便携式示波器",null,"套",2,null,""]
[-2,"数字万用表",null,"套",2,null,""]
[-3,"频率计",null,"套",2,null,""]
[-4,"网络通断测试仪",null,"套",2,null,""]
[-5,"套装维修工具",null,"套",2,null,""]
[-6,"地阻表",null,"套",2,null,""]
[-7,"笔式逻辑器",null,"套",2,null,""]
[-8,"专用键盘",null,"个",2,null,""]
[-9,"复合通行卡读写器",null,"套",2,null,""]
[-10,"收据打印机",null,"台",2,null,""]
[-11,"费额称重显示器",null,"套",2,null,""]
[-12,"手动栏杆",null,"套",2,null,""]
[-13,"自动栏杆臂",null,"根",2,null,""]
[-14,"移动硬盘","2TB","套",2,null,""]
[-15,"车道控制器",null,"台",2,null,""]
[-16,"广场摄像机",null,"台",1,null,""]
["900-4","供电照明",{"$nulls":4},""]
["900-4-2","供配电设施",{"$nulls":4},""]
[-1,"箱式变电站   100KVA",null,"套",3,null,"","含基础和接地装置"]
[-2,"箱式变电站   315KVA",null,"套",3,null,"","含基础和接地装置"]
[-3,"柴油发电机组 150KW",null,"套",1,null,"","含基础和接地装置"]
[-4,"柴油发电机组 120KW",null,"套",2,null,"","含基础和接地装置"]
[-5,"柴油发电机组 50KW",null,"套",1,null,"","含基础和接地装置"]
["900-4-3","照明设施",{"$nulls":4},""]
[-1,"路灯 12米高、200W LED灯",null,"基",4,null,"","含基础和接地装置"]
[-2,"路灯 15米高、2*180W LED灯",null,"基",4,null,"","含基础和接地装置"]
[-3,"30m 升降式高杆灯、10*1kW高压钠灯",null,"基",12,null,"","含基础和接地装置"]
[-4,"大棚照明灯具 70W LED灯",null,"套",88,null,"","含安装附件"]
[-5,"广场照明配电箱(δ2mm厚镀锌钢板喷塑或不锈钢制作)",null,"套",6,null,"","含避雷器、断路器、接触器等"]
["900-4-4","电力电缆",{"$nulls":4},""]
[-1,"电力电缆  YJV-8.7/15KV-3×70",null,"m",580,null,"","以实际发生量计，含电缆接头等"]
[-2,"电力电缆  YJV-8.7/15KV-3×50",null,"m",580,null,"","以实际发生量计，含电缆接头等"]
[-3,"电力电缆 YJV-3x185+1x95",null,"m",450,null,"","以实际发生量计，含电缆接头等"]
[-4,"电力电缆  YJV-4×16",null,"m",520,null,"","以实际发生量计，含电缆接头等"]
[-5,"低压供电电缆  YJV-4×25",null,"m",4260,null,"","以实际发生量计，含电缆接头等"]
[-6,"低压供电电缆  YJV-4×16",null,"m",2770,null,"","以实际发生量计，含电缆接头等"]
[-7,"低压供电电缆  YJV-4×10",null,"m",1750,null,"","以实际发生量计，含电缆接头等"]
[-8,"低压供电电缆  YJV-4×6",null,"m",560,null,"","以实际发生量计，含电缆接头等"]
[-9,"导线  BV-3×2.5",null,"m",1816,null,"","以实际发生量计，含电缆接头等"]
[-10,"导线  BV-3×6",null,"m",1700,null,"","以实际发生量计，含电缆接头等"]
["900-4-5","安装材料",{"$nulls":4},""]
[-1,"绝缘橡胶垫 宽1m",null,"m",240,null,""]
[-2,"变电所电缆沟钢盖板  1000*900*10mm",null,"块",60,null,""]
[-3,"SC20钢管",null,"m",3516,null,""]
[-4,"电力手孔",null,"个",20,null,""]
[-5,"镀锌焊接钢管 ∅76X3.5mm",null,"m",4180,null,"","含接地，金属件热镀锌"]
["900-4-8","备品备件及专用工具",{"$nulls":4},""]
[-1,"电量表（电流、电压等）",null,"套",1,null,""]
[-2,"兆欧表（1000兆欧）",null,"台",1,null,""]
[-3,"接地摇表",null,"台",1,null,""]
[-4,"万用表",null,"台",1,null,""]
[-5,"专用电工工具",null,"套",1,null,""]
["900-5","通信管道",{"$nulls":4},""]
["900-5-1","人（手）孔",{"$nulls":4},""]
[-1,"人孔",null,"个",96,null,""]
[-2,"手孔",null,"个",124,null,""]
["900-5-2","管道工程",{"$nulls":4},""]
[-1,"敷设12孔F40/33mm硅芯管",null,"m",62212,null,""]
[-2,"敷设4孔F114x4mm镀锌钢管",null,"m",1270,null,""]
[-3,"敷设2孔F114x4mm镀锌钢管",null,"m",212,null,""]
[-4,"敷设2孔F89x3mm镀锌钢管",null,"m",1988,null,""]
["900-5-3","钢网玻璃钢管箱",{"$nulls":4},""]
[-1,"钢网玻璃钢管箱","（250*150*5mm）","m",876,null,""]
["900-5-4","制作安装托架",{"$nulls":4},""]
[-1,"管箱托架",null,"套",875,null,""]
["900-5-5","混凝土包封",{"$nulls":4},""]
[-1,"C20混凝土包封",null,"m3",3098,null,""]
["900-5-6","土方",{"$nulls":4},""]
[-1,"挖土方",null,"m3",20942,null,""]
[-2,"填土方",null,"m3",17394,null,""]
["清单  第900章合计  人民币(元)",{"$nulls":5},0]

{"sheet":"汇总表","index":10,"n_rows":19,"n_cols":4,"rows_kept":19,"merged":[[0,0,0,3],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2]],"flags":["formulas_cached_only"]}
["5.4 投标报价汇总表"]
[]
["合同段编号：ZAZCB",null,null,"货币单位：人民币元"]
["序号","章次","科 目 名 称","金额(元)"]
[1,100,"总则",""]
[2,200,"路基",0]
[3,300,"路面",0]
[4,400,"桥梁、涵洞",0]
[5,500,"隧道",0]
[6,600,"安全设施及预埋管线",0]
[7,700,"绿化及环境保护设施",0]
[8,800,"房建工程",0]
[9,900,"机电工程",0]
[10,"第100章～900章清单合计",null,0]
[11,"已包含在清单合计中的材料、工程设备、专业工程暂估价合计",null,0]
[12,"清单合计减去材料、工程设备、专业工程暂估价合价\n(即10-11)=12",null,""]
[13,"计日工合计",null,0]
[14,"暂列金额（本项目不予考虑）",null,0]
[15,"投标报价(10+13+14)=15",null,""]